	
How to Use S7 Software Updater

¢º Software Updating Program for 72/702/703 Series


	Requirements 

  PC - Desktop or Notebook with the Microsoft Windows OS(Operating System) 

  Samsung Satellite Receiver (Set-top Box): 72/702/703 Series 

  RS-232C Serial Cable: 
[image: image1](1) The both ends of the cable need to be in "Female Type" 
[image: image2](2) As per the below drawing, the second and the third pin need to be crossed.
    [image: image3.png]



  Samsung STB Updater for 72/ 702 / 703 Series:
[image: image4](1) Install the program by running "SETUP.exe" after you have unzipped the file.
[image: image5](2) Upon the installation, "STB Update 2001.exe" and "STB Updater 2001 Helper.hlp"
        will be created.
[image: image6](3) Run "STB Updater 2001.exe" and follow the instructions give below to update
        the software.


Database Download 
 

DESCRIPTION
 

  STEP 1
  Press "Menu" on the remote control unit
[image: image7.png]



  STEP 2
  Go to "Installation" in the main menu
 

  STEP 3
  Select "System Setup"
 

  STEP 4
  Go to "Database Download"
 

Description
Icons to Use
  PC ¢¡ STB (From PC to Samsung digital satellite receiver) 
1. Run "STB Updater 2001.exe"
 

2. Click "File Open" icon and choose the file (*.sdb) that
    will be used to update the database
[image: image8.png]



3. Choose any of the icon indicated on the right
[image: image9.png] Send DB to STB



or[image: image10.png]



4. Choose the "1. Receive DB from PC" menu in the
   "Database Download" menu from the TV monitor and
    press "OK" button on remote control unit
[image: image11.png]



5. Click the "Send" button in the computer monitor
[image: image12.png]



  STB ¢¡ PC (From Samsung digital satellite receiver to PC) 
1. Run "STB Updater 2001.exe"
 

2. Click "File Open" icon and choose the file (*.sdb) that
    will be used to update the database
[image: image13.png]



3. Choose any of the icon indicated on the right
[image: image14.png] Receive DB from STB



or[image: image15.png]



4. Choose the "2. Send DB to PC" menu in the
    "Database Download" menu from the TV monitor and
    press "OK" button on remote control unit
[image: image16.png]



5. Click the "Receive" button in the computer monitor
[image: image17.png]



  STB ¢¡ STB (From Samsung digital satellite receiver to another Samsung receiver) 
1. Connect the Samsung receivers with RS232C cable.
[image: image18.png]



2. Switch on the power of both receivers, and go to
   "Database Download" menu.
 

3. Choose "3. Receive DB from STB" or "4. Receive DB to
    STB" according to the role of each receiver. (e.g. the STB
    sending the database need to be in "3. Receive DB from
    STB" menu.
 

4. Press the "OK" button on the receiver separately or
    simultaneously
 

5. Check the LED on the STB or the bar indicating the
    progress on the TV monitor
 


Program Update 

1. Unplug the power cord of your Samsung digital satellite receiver. [image: image19.png]



2. Connect the RS-232C serial cable to COM 1 port of your computer. 

3. To prevent any unexpected failure, please close the programs, if any, running on COM1 port of your PC, especially the HyperTerminal. 

4. Connect the remaining connection jack of RS-232C serial cable to your Samsung satellite receiver. 

5. Run "STB Updater 2001.exe" 

6. Click the [image: image20.png]


(file open) button and select the file (*.ser) that will be used for update your receiver's program. 

7. Select COM Port by clicking the icon "[image: image21.png]


". (Default: COM1 / 115200bps) 

8. Click "Update" button ( [image: image22.png]


) to initiate the progress. 

9. Plug the power cord of your Samsung set-top box and press the " [image: image23.png]


" button on the front panel, if necessary. [image: image24.png]



10. The below dialogue box would appear if the above procedure was accompanied properly.
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11. On completion of data transmission, the message of "Completed Successfully" should appear. Please unplug the RS-232C cable connected to your STB afterwards. 

12. Unplug the power cord of your set-top box and re-plug it after few seconds. The box will reboot with new software. 

13. If you should update any other Samsung STB please follow the above procedures again. 


Commonly Asked Questions 
1. If the below message should appear after clicking any of "Send/Receive/Update" buttons, 
please run the "STB Updater 2001" program again. If the same message should appear please check and close the programs that are running, especially the HyperTerminal.

[image: image26.png][Errorl]: COM Port!
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2. If you are run the program again after you have cancelled or stopped during the "Program Update", please restart from the beginning following the same procedure.

3. If the following error message appear on the screen "file size is wrong", after you have clicked either the "Send" or "Update" button of "STB Updater 2001" program, please check if the file you have downloaded from the homepage is bigger than 0KB. If not please download it again.





